laminarflow_to              .40
laminarflow_cruise          .40
laminarflow_loiter          .40
laminarflow_landing         .40


M_cruise            0.8
M_to                0.2
M_loiter            0.3
M_landing           0.2

cLalpha             0.057
cL0                 0.144
cMalpha             -.066
cM0                 -0.211

efficiency_to       0.8
efficiency_cruise   0.8
efficiency_loiter   0.8
efficiency_landing  0.8

alt_cruise          35000
alt_to              0
alt_loiter          10000
alt_landing         0

weight_cruise       160000
weight_to           160000
weight_loiter       130000
weight_landing      130000

cd_correction       0
c_f                 0.003